

Partnership Courtyard, The Ramparts,

Dundalk, Ireland

Version 6.8.0.0

March 7, 2022

www.measuresoft.com

+353 42 933 2399

This document is the copyright of Measuresoft and may not be modified, copied or distributed in any form whatsoever without the prior permission of Measuresoft.

Agilent Power Supplies User Manual

Table of Contents

1 Configuration 3

2 Advanced Device Configuration 4

2.1 AutoEnable Device 4

2.2 Scan Rate 4

2.3 Save Outputs 4

2.3.1 By Tag 4

2.4 Device Specific Button 5

2.4.1 Model 5

2.4.2 ProLogix Ethernet GPIB 5

2.4.2.1 Lan Address 5

2.4.2.2 GPIB Address 5

2.4.3 NI GPIB 5

2.4.3.1 Board Address 5

2.4.3.2 GPIB Address 5

2.4.4 LAN 5

2.4.4.1 Lan Address 5

2.4.5 Command 5

3 Analog Output Channel Configuration 7

3.1 Enable Channel 7

3.2 Tag 7

3.3 Description 7

3.4 Engineering Units 8

3.4.1 Minimum 8

3.4.2 Maximum 8

3.4.3 Descriptor 8

3.5 Device Specific Button 8

3.5.1 Output Type 8

4 Digital Output Channel Configuration 9

4.1 Enable Channel 9

4.2 Tag 9

4.3 Description 9

4.4 Low State Description 10

4.5 High State Description 10

4.6 Event Checking 10

4.7 Alarm Checking 10

4.7.1 Alarm State 10

4.7.2 Alarm Priority 10

4.7.3 Common Alarm 10

4.7.4 Alarm Delay 10

4.7.5 Alarm Message 10

4.8 Device Specific Button 10

4.8.1 Output Type 11

# Configuration

The first time the system is configured it is necessary to enable and configure all devices you require. To configure a particular device select the ***Devices*** option from the main menu followed by the Agilent Power Supplies device. This will launch an application to configure the device.

From the list provided select a channel and double-click. Alternatively you can select a channel and then click on the Configure Channel button. 

This will launch a channel configuration dialog which enables you to configure individual channels.



# Advanced Device Configuration



## AutoEnable Device

To ensure that the device is enabled on the system check the Enable Device box.

## Scan Rate

To set the rate at which the device will scan, edit the text boxes associated with the Scan Rate field.

## Save Outputs

To enable this utility check the Save Outputs flag. All values in output channels are saved to disk when the system is disabled. The next time the system is restarted the values which were previously in output channels will be restored to the appropriate channel number.

### By Tag

Channel values can be saved and restored to channels using the channel tag instead of the channel number. In this way, channels can be rearranged within the modules and as long as the channel tags remain the same, the correct channel values will be restored to the appropriate channel number.

## Device Specific Button

When the Device Specific Button is pressed the following dialog appears to allow specific communication settings to be configured for the device.



### Model

The model can be set to one of the following

6033

5700

### ProLogix Ethernet GPIB

This option used to establish a link to the device via ProLogix GPIB Ethernet converter.

#### Lan Address

Displays IP address or name of the ProLogix unit

### NI GPIB

This option used to establish a link to the device via National Instruments GPIB devices.

#### Board Address

Address of the NI device.

#### GPIB Address

This is the GPIB address of the Agilent unit.

### LAN

This option used to establish a direct Ethernet link to a 5700 device devices.

#### Lan Address

Displays IP address or name of the Agilent 5700 device

### Command

The command button is used to launch the send command dialog to communicate directly with the device.



# Analog Input and OutputChannel Configuration

Current Analog Outputs values are read from the device when the scanning starts. If the output changes on the device e.g. from the front panel the new value is read into channels. If the output changes via system channels e.g. from the calculator or a monitor the output is written to the device.

When the user selects an analog output to be configured the following is displayed.



## Enable Channel

The Enable Channel check box must be checked to enable and allow a channel to be configured and ultimately included with all other configured channels in the overall system.

## Tag

The Tag field is a 12 character alphanumeric field that can contain channel information or wiring schedule references.

## Description

The Description field is a 32 character alphanumeric field in which a description of the channel can be detailed.

## Engineering Units

Specifies engineering details for this channel.

Minimum

Minimum engineering value for all Analog channels in addition to the unit field. The default is 0.

Maximum

Maximum engineering value for all Analog channels in addition to the unit field. The default is 100.

Descriptor

Describe the units of the measurement.

## Device Specific Button

When the Device Specific Button is pressed the following dialog appears to allow specific device configuration of the particular channel.





### GPIB Address

GPIB Addess of the Agilent unit.

### Input Type

Specifies if output is voltage or current..

### Output Type

Specifies if output is voltage or current, voltage high limit or voltage low limit. Voltage low limit is not supported on the 6033 models.

# Digital Output Channel Configuration

Current Digital Outputs values are read from the device when the scanning starts. If the output changes on the device e.g. from the front panel the new value is read into channels. If the output changes via system channels e.g. from the calculator or a monitor the output is written to the device.

When the user selects a digital output to be configured the following is displayed.



## Enable Channel

The Enable Channel check box must be checked to enable, and allow this channel to be configured and ultimately included with all other configured channels in the overall system.

## Tag

The Tag field is an 12 character alphanumeric field that can contain channel information or wiring schedule references.

## Description

The Description field is a 32 character alphanumeric field in which a description of the channel can be detailed.

## LowState Description

A 32 character field in which to enter a description of the low state of the channel.

## HighState Description

A 32 character field in which to enter a description of the high state of the channel.

## Event Checking

Event checking is used, if required to trigger a logger to record information on an event. If this facility is required click on the drop down list box and select OFF, HIGHSTATE, or LOWSTATE as appropriate. Events are detected on inputs using data acquired at 1Khz. Events are detected on outputs using the configured scan rate.

## Alarm Checking

### AlarmState

Alarm checking is available on all channels throughout the system. To configure alarm checking on this channel click on the drop down box and select OFF, HIGHSTATE, or LOWSTATE as appropriate. If the channel's output state changes to an AlarmState an alarm will be triggered on the channel. When monitoring channels, if the alarm is triggered, the fact will be annotated alongside the other channel information in the Channel Monitor . Alarms and warnings are detected at the configured scan rate.

### Alarm Priority

Enter the priority of the alarm triggered by this channel. Alarm priority ranges are from 0 to 255.

### Common Alarm

Channels can be configured to trigger a Common Alarm. A common alarm is a single digital output which will switch on when any channel with the Drive Common Alarm enabled goes into an alarm state.

### Alarm Delay

Enter the time, in seconds, between the channel value entering the alarm state and the system flagging an alarm.

### Alarm Message

An Alarm Message can be defined to be displayed on the Status line of the Main Window when a channel goes into an alarm state.

## Device Specific Button

When the Device Specific Button is pressed the following dialog appears to allow specific device configuration of the particular channel.



### Output Type

This can be set to the Output status to enable (HIGH STATE) to disable (LOW STATE) the output.

This can be set to the Front Panel Lock to lock (HIGH STATE) to unlock (LOW STATE) the front panel. This is not available on the 6033.

This can be set to the Current Protection to enable (HIGH STATE) or disable (LOW STATE) over-current protection.This is not available on the 6033.