

Partnership Courtyard, The Ramparts,

Dundalk, Ireland

Version 6.4.1.2

January 27, 2017

www.measuresoft.com

+353 42 933 2399

This document is the copyright of Measuresoft and may not be modified, copied or distributed in any form whatsoever without the prior permission of Measuresoft.

Yokogawa WT 3000 Driver User Manual

Table of Contents

1 Configuration 3

2 Channel Configuration 3

2.1 Enable Channel 3

2.2 Tag 3

2.3 Description 3

2.4 Engineering Units 3

2.4.1 Minimum 3

2.4.2 Maximum 3

2.4.3 Descriptor 3

2.5 Device Specific Button 3

2.5.1 Function 3

2.5.2 Element 3

3 Advanced Device Configuration 3

3.1 AutoEnable Device 3

3.2 Scan Rate 3

3.3 Save Outputs 3

3.3.1 By Tag 3

3.4 Device Specific Button 3

3.4.1 Communication Settings 3

3.4.2 Mode 3

3.4.3 Sync Src 3

3.4.4 Frequency Filter 3

3.4.5 Line Filter 3


3.4.6 Range 3

3.4.7 Averaging 3

3.4.8 Wiring 3

3.4.9 Max Hold 3

# Configuration




The first time the system is configured it is necessary to enable and configure all devices you require. To configure a particular device select the ***Devices*** option from the main menu followed by the Yokogawa\_WT device. This will launch an application to configure the device.

From the list provided select a channel and double-click. Alternatively you can select a channel and then click on the Configure Channel button. 

This will launch a channel configuration dialog which enables you to configure individual channels.

# Channel Configuration



## Enable Channel

The Enable Channel check box must be checked to enable and allow a channel to be configured and ultimately included with all other configured channels in the overall system.

## Tag

The Tag field is a 12 character alphanumeric field that can contain channel information or wiring schedule references.

## Description

The Description field is a 32 character alphanumeric field in which a description of the channel can be detailed.

## Engineering Units

Specifies engineering details for this channel.

### Minimum

Minimum engineering value for all Analog channels in addition to the unit field. The default is 0.

### Maximum


Maximum engineering value for all Analog channels in addition to the unit field. The default is 100.

### Descriptor

A four character field available to describe the units of the measurement.

## Device Specific Button

When the Device Specific Button is pressed a dialog appears detailing the Analog Value Mapping between the channel being configured and the data associated with that channel. These settings are in relation to display configurations.



### Function

Sets display function.


### Element

Sets display element.

### Order

Sets display element order.

# Advanced Device Configuration



## AutoEnable Device

To ensure that the device is enabled on the system check the Enable Device box.

## Scan Rate

To set the rate at which the device will scan, edit the text boxes associated with the Scan Rate field.

## Save Outputs


To enable this utility check the Save Outputs flag. All values in output channels are saved to disk when the system is disabled. The next time the system is restarted the values which were previously in output channels will be restored to the appropriate channel number.

### By Tag

Channel values can be saved and restored to channels using the channel tag instead of the channel number. In this way, channels can be rearranged within the modules and as long as the channel tags remain the same, the correct channel values will be restored to the appropriate channel number.

## Device Specific Button

When the Device Specific Button is pressed the following dialog appears to allow specific communication settings to be configured for the device.



### Address

The IP Address of the WT 3000

### User Name

User name for Ethernet access to the device

### Password

Password for Ethernet access to the device. Leave password blank if using anonymouse user name,

### Command

The command button is used to launch the send command dialog to communicate directly with the device. See the WT3000 User manual for a list of commands.

