



**Measuresoft Development Ltd.**

**Ametek Programmable Power**

**VTI EX1401 User Manual**

**Version:** **6.5.0.0**

1. Installation 2

2. Configuration 3

3. Advanced Device Configuration 4

3.1 AutoEnable Device 4

3.2 Scan Rate 4

3.3 Save Outputs 4

3.4 Device Specific Button 4

3.4.1 Address 4

3.4.2 Temperature in Farenheit 5

3.4.3 Browse 5

4. Channel Configuration (Analogs) 6

4.1 Enable Channel 6

4.2 Tag 6

4.3 Description 6

4.4 Units 6

4.5 Scaling 6

4.5.1 Auto Scaling 7

4.6 Significant Change 7

4.7 Event Checking 7

4.7.1 High Limit 7

4.7.2 Low Limit 7

4.8 Alarm Checking 7

4.8.1 Enable Alarm Checking 8

4.8.2 Drive Common Alarm 8

4.8.3 Alarm Limit 8

4.8.4 Warning and Limit (Analogue channel only) 8

4.8.5 Hysteresis 8

4.8.6 Priority 8

4.8.7 Alarm Delay 8

4.8.8 Alarm Message 8

4.8.9 Alarm on Error Checking 8

4.9 Device Specific Button 8

4.9.1 Analog Inputs 9

5. Channel Configuration (Digitals) 9

5.1 Enable Channel 10

5.2 Tag 10

5.3 Description 10

5.4 Low State Description 10

5.5 High State Description 10

5.6 Event Checking 10

5.7 Alarm Checking 11

5.7.1 Alarm State 11

5.7.2 Alarm Priority 11

5.7.3 Common Alarm 11

5.7.4 Alarm Delay 11

5.7.5 Alarm Message 11

5.7.6 Alarm on Error Checking 11

# Installation

The Ametek Programmable Power EX1401 Driver installation has the following two stages:

1. Installation of the Vtex 1401 Driver, IVI, VtexDsa 32-bit or 64-bit

2. Installation of the ScadaPro Ametek Programmable Power VTI EX1401 Driver

NB: Please complete the stages above in the order indicated.

The Vtex Vtex 1401 Driver, IVI, VtexDsa 32-bit or 64-bit can be downloaded from https://www.powerandtest.com/ate-data-acq/platforms/lxi/ex1400-family/ex1401.

Install the ScadaPro Ametek Programmable Power VTI EX1401 driver from the installation CD provided by running the driver setup.msi. Accept the default installation settings.

# Configuration


The first time the system is configured it is necessary to enable and configure all devices you require. To configure a particular device select the ***Devices*** option from the main menu followed by the appropriate device.

This will launch an application to configure the device. You will be presented with a set of tab dialogs as shown above.

The Advanced device configuration is used to configure the device IP addeess.

To configure channels, click on the appropriate channel tab. From the list provided select a channel and double-click. Alternatively you can select a channel and then click on the ***Configure Channel*** button. This will launch a channel configuration dialog which enables you to configure individual channels.

# Advanced Device Configuration



## AutoEnable Device

To ensure that the device is enabled on the system check the Enable Device box.

## Scan Rate


To set the rate at which the device will sample, edit the text boxes associated with the Scan Rate field. Setting the Mins Sec and Ms to 0 allows input of a sampling frequency.

## Save Outputs

To enable this utility check the Save Outputs flag. All values in output channels are saved to disk when the system is disabled. The next time the system is restarted the values which were previously in output channels will be restored to the appropriate channel number.

## Device Specific Button

If the Device Specific Button is visible, then click on it to configure features that are specific only to this device. In the case of EX1401 the following dialog will appear.



### Address

The IP address of the EX1048 device

### Temperature in Fahrenheit


Temperature in Fahrenheit. Report temperatures in degrees Celsius or degrees Fahrenheit.

### Browse

Browse is used to open the Internet Bowser to access the EX1048 device directly.

# Channel Configuration (Analogs)

Physical Analog Input Channel 1 to 16 are mapped to analog inputs 1 to 16.



## Enable Channel

The Enable Channel check box must be checked to enable, and allow this channel to be configured and ultimately included with all other configured channels in the overall system.

## Tag

The Tag field is a 12 character alphanumeric field that can contain channel information or wiring schedule references.

## Description

The Description field is a 32 character alphanumeric field in which a description of the channel can be detailed.

## Units

A 4 character field available to describe the units of the output.

## Scaling

NB. Scaling is only available to Analog channels that are not Output channels.

Some transducers give a number of pulses, or a frequency output proportional to their full scale range. To enable the Scaling utility check the Scaling Check box. The Slope and Offset values can be entered directly into the text boxes. The formula applied is:

y = mx + c where: m is SLOPE

x is the measured value.

c is the OFFSET

### Auto Scaling

Click On the Auto Scale button if you want the scale and offset values calculated automatically. A dialog box will be displayed. Enter the values in the text boxes. The low measured value, and the high measured value, the output range of the transducer. When the fields have been completed, and assuming the System is enabled click on the Apply button. Under the heading Current Values the actual measured value will be shown, as well as the Engineering Value.

Click on OK to accept the scaling, or Cancel to abort the Auto Scaling feature.

NB. Scaling will not be applied to the channel, even if the system is enabled, until the system is next enabled or the Device is reconfigured

## Significant Change

To enable the Significant Change feature check the Sig Change check box. This facility allows filtering of data on channels on which significant change is of interest. Such changes can cause an event, which can be logged.

The figure entered in the Value text box, is the rate of change that if the output level exceeds per scan, either increasing or decreasing will cause the significant change event trigger. The scan rate is determined in the Advanced Device configuration

If a logger is configured each time the significant change trigger operates information on the channels defined in the logger will be recorded . A significant change event only lasts one scan, unless the next reading also changes greater than the Significant change value

When monitoring channels, if the Significant Change is triggered, then the fact will be annotated alongside the other channel information in the Channel Monitor. The significant change events are in addition to those caused by an Event.

## Event Checking

Event checking is used, if required to trigger a logger to record information on a number of channels during an event. Check the Event Checking check box if this channel is to trigger an event.

### High Limit

A value, in engineering units, entered in this text box will define the level that, if exceeded, will cause an event trigger.

### Low Limit

A value entered in this text box will define the level that if the channel result falls below will cause an event trigger.

## Alarm Checking

Alarm checking is available on all channels throughout the system. Low Alarm and High Alarm levels can be configured independent of each other. If the channel output exceeds the High Alarm limit then an alarm will be triggered as it will if the output goes below the Low Alarm limit.

When monitoring channels, if the high or low alarm is triggered, then the fact will be annotated alongside the other channel information in the Channel Monitor. To configure the Alarm Checking section of the device complete the options as follows for either or both the High Alarm and Low Alarm checking.

### Enable Alarm Checking

Check either the Low Alarm Checking or High Alarm Checking or both check boxes to enable the facility.

### Drive Common Alarm

A common alarm is a single digital output which will switch on when any channel with the Drive Common Alarm enabled goes into an alarm state. Check this box if a link to the Common Alarm is required.

### Alarm Limit

Specifies the value which will trigger this alarm. for Low Alarm Checking it will be any value <= the Alarm Limit and for High Alarm Checking it will be any value >= the Alarm Limit.

### Warning and Limit (Analogue channel only)

If required, a warning can be displayed when a channel reaches a limit close to the alarm limit. For low alarm checking, the limit must be less than the alarm limit. For high alarm checking, the warning limit must be less than the alarm limit

### Hysteresis

Hysteresis can prevent 'noisy' channels from reporting multiple alarms when the average reading is close to the alarm threshold. Check the box if this feature if needed. Enter the value of the dead band in the corresponding value field.

### Priority

Enter or edit the number in the text box to allocate the priority of this alarm. Alarm priority ranges are from 0 to 255.

### Alarm Delay

Enter the time, in seconds, between the channel value entering the alarm state and the system flagging an alarm.

### Alarm Message


An Alarm Message can be defined to be displayed on the Status line of the Main Window when a channel goes into an alarm state. Enter the message, up to 32 characters, that is to appear in the event of an alarm.

### Alarm on Error Checking

Checking this section will enable the device to generate alarms when a channel goes into error.

## Device Specific Button

When the Device Specific Button is pressed the following dialog is presented.



### Analog Inputs

#### EU Conversion

Sets the engineering units (EU) conversion for the channel.

#### Range

Sets the measurement range for the specified channels

#### User Defined CJC Temperature


Enables the use of a user-defined CJC temperature instead of the internally measured one.

#### CJC Temperature

Sets the user-defined CJC temperature for the channel. The value is entered in Degrees Celsius regardless of whether results are reported in Fahrenheit or Celsius.

# Channel Configuration (Digitals)

DIO Channels 0 to 7 are mapped to digital outputs 1 to 8.



## Enable Channel

The Enable Channel check box must be checked to enable, and allow this channel to be configured and ultimately included with all other configured channels in the overall system.

## Tag

The Tag field is a 12 character alphanumeric field that can contain channel information or wiring schedule references.

## Description

The Description field is a 32 character alphanumeric field in which a description of the channel can be detailed.

## Low State Description

A 32 character field in which to enter a description of the low state of the channel.

## High State Description

A 32 character field in which to enter a description of the high state of the channel.

## Event Checking

Event checking is used, if required to trigger a logger to record information on an event. If this facility is required click on the drop down list box and select OFF, HIGH STATE, or LOW STATE as appropriate

## Alarm Checking

### Alarm State

Alarm checking is available on all channels throughout the system. To configure alarm checking on this channel click on the drop down box and select OFF, HIGH STATE, or LOW STATE as appropriate. If the channel's output state changes to an Alarm State an alarm will be triggered on the channel. When monitoring channels, if the alarm is triggered, the fact will be annotated alongside the other channel information in the Channel Monitor .

### Alarm Priority

Enter the priority of the alarm triggered by this channel. Alarm priority ranges are from 0 to 255.

### Common Alarm

Channels can be configured to trigger a Common Alarm. A common alarm is a single digital output which will switch on when any channel with the Drive Common Alarm enabled goes into an alarm state.

### Alarm Delay

Enter the time, in seconds, between the channel value entering the alarm state and the system flagging an alarm.

### Alarm Message

An Alarm Message can be defined to be displayed on the Status line of the Main Window when a channel goes into an alarm state.

### Alarm on Error Checking

Checking this section will enable the device to generate alarms when a channel goes into error.

## 

be created on the same input channel and/or spanning multiple input channels.