Wiring For Mitsubishi : 9 Pin

2,3 - Switched

1,4,6 - Looped Out

7,8 - Looped Out

5 - Straight Through

9 - Straight Through