Wiring For Mitsubishi : 9 Pin

 2,3 - Switched

 1,4,6 - Looped Out

 7,8 - Looped Out

 5 - Straight Through

 9 - Straight Through